460 Yield Steel Plate

1. Designers are increasingly using 460 MPa yield plate to combine increased strength with savings in weight.

With availability in both structural and pressure vessel grades in a wide range of plate sizes and thicknesses. Steel can be supplied as plates, cut plates, or profiles (cut to shape).

2. We recognise the need for an ex-stock source of 460 yield plate and are able to offer the following material:

EN 10028-3 P460NL1

EN 10028-3 P460NL2

EN 10028-3 P460NH

EN 10025-3 S460N

EN 10025-3 S460NL

3. Applications

Bridges

Grouted tees/Grouted sleeves

Pipe caps/Pipe fittings

Pipe lines

Plate girders

Pressure vessels

Road tankers

4. If you have any other requirement for steel plate, please feel free to contact us.