ASTM A537 CL1 CL2 CL3 Steel Plate Supplier

1. A537 plate steel is heat-treated. As a result, it displays greater yield and tensile strength than the more standard A516 grades. A537 steel plate is ideal for both in boilers and pressure vessels, and is used in the oil, gas and petrochemical industry.

|  |  |  |  |
| --- | --- | --- | --- |
| PVQ Pressure Vessel Steel Plate | | | |
| all measurement in Inches | Thickness | Width | Length |
| A537 | 1/2" – 4" | 48" – 120" | 96" – 480" |

2. If you have any other requirement for steel plate, please feel free to contact us.