EN 10028:2 P265GH STEEL PLATE

1. Stocks of boiler plate steel ready to be supplied as plate, cut plate, or profiles (cut shapes) and certified to EN 10028:2 P265GH are available.

2. EN 10028:2 P265GH

The specification EN 10028:2 covers a range of non-alloy and alloy steels with specified elevated temperature properties intended for pressure purposes. EN 10028:2 P265GH is steel for pressure purposes (P) with minimum yield strength of 265 MPa (265). We are also stockists of EN 10028:3 plates manufactured and certified to:

EN 10028:3 P355NL1      EN 10028:3 P355NL2

EN 10028:3 P355NH       EN 10028:3 P275NH

3. If you have any other requirement for steel plate, please feel free to contact us.