SA537 Class 1 STEEL PLATE

We are also world-leading stockists and processors of other ASME and ASTM carbon steel pressure vessel plates manufactured and certified to:

ASTM A516 Gr. 70 ASME SA516 Gr. 70

ASTM A516 Gr. 65 ASME SA516 Gr. 65

ASTM A516 Gr. 60 ASME SA516 Gr. 60

ASTM / ASME A / SA 516 Gr. 60 / 65 / 70 HIC

The A537 / SA537 standard, its full name is “Standard Specification for Pressure Vessel Plates, Heat-Treated, Carbon-Manganese-Silicon Steel”, is intended use in the manufacture of fusion welded pressure vessels and structures.

The material under this specification is available in three classes. Class 1 steel is supplied in the normalised condition and the specification covers plates up to 100 mm (4 inches) in thickness.

If you have any other requirement for steel plate, please feel free to contact us.