API 2H Gr50 Offshore & Structural Steel Plate

Supplied in as rolled, normalised, and quenched and tempered condition as applicable, UNITEDSTEEL carries a wide range of structural and offshore steel plate to satisfy offshore contractors and steel fabricators in a full range of plate sizes up to 20 m long and 4 m wide in the thickness range 3 mm to 340 mm.

From the most basic structural grade through to highly specialised project related specifications, steel is available shot blasted and primed from stock and can be cut to size.

We can provide a complete project service, with fast track mill service available – for distribution worldwide.

Specifications

BS EN 10025

S235, S275, S355, S420, S460, S690, S890, S960

BS EN 10225

S355, S420, S460

API 2H Gr50

ASME/ASTM SA/A 36, 283 Gr C, 285 Gr C, 572 Gr 50

Applications

Bridges

Machinery Parts

Mechanical Engineering

Mining Equipment

Oilfield Fabrications

Plate Girders

Transport Equipment

Storage Tanks

Wind Towers

If you have any other requirement for steel plate, please feel free to contact us.