API 2H Grade 50 Steel Plate

1. API 2H Steel Plate Grade 50 is an intermediate-strength, normalized, structural-steel plate used in the welded construction of offshore structures in critical portions. Steel used in these applications must exhibit higher impact toughness and resistance to fatigue loading. It is regulated by the American Petroleum Institute and in some cases, certified by ABS (American Bureau of Shipbuilding).

|  |
| --- |
| Offshore & Marine Steel Plate |
| all measurement in Inches | Thickness | Width | Length |
| API 2H | Grade 50 | 1/2" – 4" | 48" – 120" | 96" – 480" |

2. If you have any other requirement for steel plate, please feel free to contact us.