A830-1020 Steel Plate

1. High-Carbon A830-C1020 steel plate is of structural quality grade plate. C1020 provides greater strength and hardness levels. These plates are usually supplied in the as-rolled (hot-rolled) condition.

|  |
| --- |
| Low/High Carbon Non Structural Steel Plate |
| all measurement in Inches | Thickness | Width | Length |
| A830–C1020 Carbon Steel Plate | 1/4" – 3" | 48" – 120" | 96" – 480" |

2. If you have any other requirement for steel plate, please feel free to contact us.