ABS Gr AH36 Steel Plate

1. China United Iron and Steel Limited offers grades that are certified by ABS (American Bureau of Shipbuilding) and represents the Higher Strength Group of ABS steel plate grades AH36, DH36 and EH36. Like ABS steel plate grade A & grade B, these grades of steel plate are almost exclusively utilized in the shipbuilding industry for the construction of structural parts of ships, barges and marine equipment.

2. China United Iron and Steel Limited stocks AH36 in the control-rolled condition, DH36 in both the control-rolled and normalized condition, and EH36 in the normalized condition.

|  |
| --- |
| Offshore & Marine Steel Plate |
| all measurement in Inches | Thickness | Width | Length |
| ABS | Grade 55 | 3/16" – 6" | 48" – 120" | 96" – 480" |
| Grade 60 | 3/16" – 6" | 48" – 120" | 96" – 480" |
| Grade 65 | 3/16" – 6" | 48" – 120" | 96" – 480" |
| Grade 70 | 3/16" – 6" | 48" – 120" | 96" – 480" |

3. If you have any other requirement for steel plate, please feel free to contact us.