AR200, AR235 Steel Plate Supplier

1. AR Medium steel plate can be ordered to AR200 or AR235 depending on the producing mill’s capabilities. AR Medium is used to cover carbon-manganese steel plates in order to provide abrasion resistance that is superior to most structural-quality carbon steels.

2. AR Medium steel plates are intended for moderate wear applications, offering improved wear resistance over an as-rolled, structural carbon steel.

3. AR Medium plates are not intended for structural applications and should not be used for structural or main load-bearing members.

|  |
| --- |
| Abrasion Resistant Steel Plate |
| all measurement in Inches | Thickness | Width | Length |
| AR235/AR Medium | 3/16" – 3/4" | 48" – 120" | 96" – 480" |

4. If you have any other requirement for steel plate, please feel free to contact us.