AR400,AR400F Steel Plate

1. AR400F plate from China United Iron and Steel Limited combines through-hardness and toughness with superior flame cutting, forming, & welding characteristics. With a typical BHN hardness of 360 – 440, this user-friendly grade permits more latitude in design and fabrication for the end user.

2. AR400F steel plates are suitable for applications that require a good level of abrasion resistance such as bucket components, construction equipment, and wear plates used in a variety of industries like mining, forestry and construction. This product will last up to four times longer than ordinary high-strength structural plate.

Each producing mill has its own proprietary chemical composition and heat-treating process.

|  |  |  |  |
| --- | --- | --- | --- |
| Abrasion Resistant Steel Plate | | | |
| all measurement in Inches | Thickness | Width | Length |
| AR400F | 3/16" – 4" | 48" – 120" | 96" – 48 |

3. If you have any other requirement for steel plate, please feel free to contact us.