SA387 / A387 Grade 11 Class 2

UNITEDSTEEL holds stocks of chrome moly pressure vessel plate for high temperature purposes certified to ASTM A387 Grade 11 Class 2 and ASME SA387 Grade 11 Class 2. Plates can also be supplied cut to size or flame cut to specific shapes.

If you have any other requirement for steel plate, please feel free to contact us.