SA387 / A387 Grade 12 Class 2 STEEL PLATE

Chrome moly pressure vessel plate for high temperature purposes certified to ASTM A387 Grade 12 Class 2 and ASME SA387 Grade 12 Class 2 is available from UNITEDSTEEL can be supplied as cut shapes or simply cut to a smaller size.

If you have any other requirement for steel plate, please feel free to contact us.