SA387 / A387 Grade 22 Class 2 STEEL PLATE

Plate certified to ASTM A387 Grade 22 Class 2 and ASME SA387 Grade 22 Class 2 is available fromReliable. These grades of steel are chrome moly pressure vessel plates for high temperature applications. As well as supplying in plate form, it can cut plates to size and also cut to specific shapes.

If you have any other requirement for steel plate, please feel free to contact us.