140 ksi Steel Plates

1. 140 ksi steel plate & 960 MPa is a high-strength, structural grade plate steel used in applications that require greater design strength. 140 ksi offers a higher min-yield (140 ksi) and tensile strength (142 ksi), combined with good toughness, excellent weldability and formability. It offers opportunities for weight reduction in some applications for increased payload in the finished unit.

2. We stock a solid supply of 140 ksi, which is most often used in the manufacture of heavy equipment such as haul trailers, crane booms, truck frames, logging and construction equipment, as well as design fabrications.

|  |  |  |  |
| --- | --- | --- | --- |
| Quenched & Tempered Alloy Steel Plate | | | |
| all measurement in Inches | Thickness | Width | Length |
| 140ksi/890 MPa | 3/16" – 1/2" | 48" – 96" | 96" – 480" |

3. If you have any other requirement for steel plate, please feel free to contact us.