EN 10025:3 S460NL STEEL PLATE

460 yield structural steel plates certified to EN 10025:3 P460NL form part of Brown McFarlane's standard product range. The plates can be supplied straight from stock, cut to size, or profiled to specific shapes.

EN 10025:3

The designation EN 10025:3 S460NL shows that this is steel for structural purposes (S) with minimum yield strength at 16 mm thick and below of 460 MPa (460) and which has specified minimum impact energy values at temperatures not lower than -50 deg C (NL).

As well as S460NL we are stockists of plates to EN 10025:3 S460N

If you have any other requirement for steel plate, please feel free to contact us.