S32205 Duplex Steel Plate

UNITEDSTEEL stocks a wide range of large area duplex stainless steel plates which are certified to material grades UNS S31803, UNS S32205, and 1.4462. These steels are also compatible with the branded 2205 designation.

For more information on Duplex stainless steel and to visit our product page.

All stock is is fully certified in accordance with the relevant material specification. In addition the material is enhanced with further tests such as E562 microstructure analysis, and corrosion testing to G48 or A293 Method C. In order to further ensure good corrosion resistance, all stock is purchased with a guaranteed minimum PREN of 35.

All material is produced and certified in accordance with NORSOK MDS D45 with plates up to and including 35 mm thick certified to Revision 4. Mill test certificates are produced with third party inspection to EN 10204 3.2.

If you have any other requirement for steel plate, please feel free to contact us.